Signal Name | Total Product Terms | Product Terms | Location | Power Mode | Pin Number | PinType | Pin Use
--- | --- | --- | --- | --- | --- | --- | ---
(unused) | 0 |  | MC1 |  |  | (b) |
ram_rom_we | 1 | 2_1 | MC2 | LOW | 50 | I/O | O
(unused) | 0 |  | MC3 |  |  | (b) |
(unused) | 0 |  | MC4 |  |  | (b) |
(unused) | 0 |  | MC5 |  | 52 | I/O | I
reset_sync | 1 | 6_1 | MC6 | LOW | 53 | I/O | I
reset | 1 | 7_1 | MC7 | LOW |  | (b) | (b)
N104/N104_D2 | 1 | 8_1 | MC8 | LOW | 54 | I/O | I
$OpTx$FX_DC$501 | 1 | 9_1 | MC9 | LOW | 55 | I/O | I
turbo_rom_adr<12> | 2 | 10_1 10_2 | MC10 | LOW |  | (b) | (b)
turbo_rom_adr<11> | 2 | 11_1 11_2 | MC11 | LOW | 56 | I/O | I
centronics_data | 3 | 12_1 12_2 12_3 | MC12 | LOW | 58 | I/O | O
rom_source_is_ram | 2 | 13_1 13_2 | MC13 | LOW |  | (b) | (b)
centronics_strobe | 2 | 14_1 14_2 | MC14 | LOW | 59 | I/O | O
centronics_clk | 3 | 15_1 15_2 15_3 | MC15 | LOW | 60 | I/O | O
rom_base_bank_6 | 2 | 16_1 16_2 | MC16 | LOW |  | (b) | (b)
rom_base_bank_0__or0000/rom_base_bank_0__or0000_D2 | 2 | 17_1 17_2 | MC17 | LOW | 61 | I/O | I
$OpTx$FX_DC$517 | 2 | 18_1 18_2 | MC18 | LOW |  | (b) | (b)

Signals Used By Logic in Function Block

1. $OpTx$FX_DC$475
2. $OpTx$FX_DC$502
3. $OpTx$FX_DC$556
4. d7_ram_rom.PIN
5. data<6>.PIN
6. data<5>.PIN
7. data<4>.PIN
8. N64/N64_D2
9. adr<10>
10. adr<7>
11. adr<9>
12. centronics_clk
13. centronics_data
14. centronics_strobe
15. check_1050_6810_access_mux0001/check_1050_6810_access_mux0001_D2
16. data<7>.PIN
17. data_0_cmp_eq0002/data_0_cmp_eq0002_D2
18. phi2
19. ram_ce
20. reset
21. reset_in
22. reset_sync
23. rom_base_bank_0__or0000/rom_base_bank_0__or0000_D2
24. rom_base_bank_6
25. rom_ce
26. rom_source_is_ram
27. rw
28. turbo_centronics_clk__or0001/turbo_centronics_clk__or0001_D2
29. turbo_rom_adr<11>
30. turbo_rom_adr<12>
31. turbo_rom_adr_11__or0001/turbo_rom_adr_11__or0001_D2